These handover minimization problem instances have four types of input lines:

p < number of towers > < number of rncs > < capacity of additional rncs >

r < rnc index > < rnc capacity >

t < tower index > < tower traffic >

h < from tower index > < to tower index > < handover >


